# Appendix A:

| **Description** | **Applicable Cables** |
| --- | --- |
| Compression Connectors | 120SQMM 3C WAVECON; 185SQMM 3C WAVECON;240SQMM 3C WAVECON; |
| Breakout Glove | 120-240SQMM 3C WAVECON; 25SQMM 3C HNS CABLE; 16SQMM 1C HNS ST.LIGHT; |
| Insulation Tube | *Overall Diameter Recovered- Expanded*12 – 35 MM; 12.7 – 22.4 MM; 6.4 – 12.5 MM ;16 – 51 MM; 38 – 75 MM (Red); 38 – 75 MM (White)38 – 75 MM (Blue); 3 – 10 MM; 4.8 – 9.5 MM |
| Zipper Sleeve | *Applicable Cables (O/A Dia Range)*35-240SQMM 1C XLPE CABLE REPAIR;OR EQUIVALENT O/A DIA 25-75MM |
| Straight Joint Kit for XLPE Cables | 185-240SQMM 3C WAVECON;120SQMM 3C WAVECON; |
| Breach Joint Kit for LV Distribution and Service Cables | 120/120 & 120/185 & 185/185SQMM 3C WAVECON;240/240SQMM 3C WAVECON; OR120-240SQMM 1X 3C PILC / 240SQMM WAVECON10/16SQMM 1C SERVICE CABLE; |
| Transition Joint for LV Consac | 120-300SQMM CONSAC AL SHEATH 3C CABLE; 120-240SQMM XLPE INSL CWN 3C CABLE185-240SQMM 3C WAVECON; 120SQMM 3½C CU STRANDED CABLE; |
| Tee- off Joint for XLPE or Paper Insulated Cables | 120-185SQMM WAVECON MAIN, 2X 25SQMM 3C XLPE BRANCH CABLE;240SQMM WAVECON MAIN, 2X 25SQMM 3C XLPE BRANCH CABLE;240SQMM 4C PLY(E) W/120SQMM NEUTRAL MAIN, 25SQMM 3C XLPE BRANCH;150SQMM 4C PLY(E) W/70SQMM NEUTRAL MAIN, 25SQMM 3C XLPE SERVICE;70SQMM 4C PLY(E) MAIN W/25SQMM NEUTRAL; 25SQMM 3C XLPE SERVICE; |
| Transition Joint for XLPE and LV Paper Insulated Cables | 240SQMM PILC; 240SQMM 3C WAVECON; |
| Straight Joint for LV XLPE Cables  | 10-16SQMM 1C SERVICE CABLE;25SQMM 3C SERVICE CABLE; |
| Termination Kit for Pole Termination | 95SQMM LV ABC; 120SQMM 3C WAVECON;150SQMM LV ABC; 185SQMM 3C WAVECON;150SQMM LV ABC; 240SQMM 3C WAVECON; |
| Pillar and Transformer Kit | 25SQMM 3C XLPE CABLE;120-240SQMM WAVECON; |
| Pit Termination Kits | 6-25 SQMM 1C PVC AND XLPE CABLE;10 & 16 SQMM 1C PVC CABLE; |
| End Caps | 25SQMM 3C HNS XLPE CABLE (23-30MM);10-16SQMM 1C SERVICE CABLE (11-16MM);150SQMM LVABC (20-26MM);95SQMM LVABC (16-22MM); |
| Heat Shrinkable End Caps | *Applicable Cables (O/A Dia Range)*CORES OF 120-240SQMM WAVECON (15-35MM);120SQMM 3C LV CABLE & 35-185SQMM HV CABLE (25-55MM);185-240SQMM 3C LV CABLE & 240-400SQMM 1C HV CABLE (32-75MM);35-95SQMM 3C HV CABLE (45-100MM) |
| Live End Seals | 70-240SQMM 3C WAVECON |
| Four Way Link Box | 120-240SQMM 3C WAVECON |